PERF-C2C(1)

NAME
perf-c2c - Shared Data C2C/HITM Analyzer.

SYNOPSIS

perf c2c record [<options>] <command>
perf c2c record [<options>] — [<record command options>] <command>
perf c2c report [<options>]

DESCRIPTION

C2C stands for Cache To Cache.

The perf c2c tool provides means for Shared Data C2C/HITM analysis. It allows you to track down the cacheline contentions.

On x86, the tool is based on load latency and precise store facility events provided by Intel CPUs. On PowerPC, the tool uses random instruction sampling with thresholding feature.

These events provide: - memory address of the access - type of the access (load and store details) - latency (in cycles) of the load access

The c2c tool provide means to record this data and report back access details for cachelines with highest contention - highest number of HITM accesses.

The basic workflow with this tool follows the standard record/report phase. User uses the record command to record events data and report command to display it.

RECORD OPTIONS

-e, --event=
    Select the PMU event. Use perf c2c record -e list to list available events.

-v, --verbose
    Be more verbose (show counter open errors, etc).

-l, --ldlat
    Configure mem-loads latency. (x86 only)

-k, --all-kernel
    Configure all used events to run in kernel space.

-u, --all-user
    Configure all used events to run in user space.

REPORT OPTIONS

-k, --vmlinux=<file>
    vmlinux pathname

-v, --verbose
    Be more verbose (show counter open errors, etc).

-i, --input
    Specify the input file to process.

-N, --node-info
    Show extra node info in report (see NODE INFO section)

-c, --coalesce
    Specify sorting fields for single cacheline display. Following fields are available: tid,pid,iaddr,dso (see COALESCE)

-g, --call-graph
    Setup callchains parameters. Please refer to perf-report man page for details.

--stdio
    Force the stdio output (see STDIO OUTPUT)

--stats
    Display only statistic tables and force stdio mode.

--full-symbols
    Display full length of symbols.

--no-source
    Do not display Source:Line column.

--show-all
    Show all captured HITM lines, with no regard to HITM % 0.0005 limit.

-f, --force
    Don’t do ownership validation.

-d, --display
    Switch to HITM type (rmt, lcl) to display and sort on. Total HITMs as default.

--stitch-lbr
    Show callgraph with stitched LBRs, which may have more complete callgraph. The perf.data file must have been obtained using perf c2c record --call-graph lbr. Disabled by default. In common cases with call stack overflows, it can recreate better call stacks than the default lbr call stack output. But this approach is not full proof. There can be cases where it creates incorrect call stacks from incorrect matches. The known limitations include exception handing such as setjmp/longjmp will have calls/returns not match.

C2C RECORD

The perf c2c record command setup options related to HITM cacheline analysis and calls standard perf record command.

Following perf record options are configured by default: (check perf record man page for details)

    -W,-d,--phys-data,--sample-cpu

Unless specified otherwise with -e option, following events are monitored by default on x86:

    cpu/mem-loads,ldlat=30/P
    cpu/mem-stores/P

and following on PowerPC:

    cpu/mem-loads/
    cpu/mem-stores/

User can pass any perf record option behind -- mark, like (to enable callchains and system wide monitoring):

    $ perf c2c record -- -g -a

Please check RECORD OPTIONS section for specific c2c record options.

C2C REPORT

The perf c2c report command displays shared data analysis. It comes in two display modes: stdio and tui (default).

The report command workflow is following: - sort all the data based on the cacheline address - store access details for each cacheline - sort all cachelines based on user settings - display data

In general perf report output consist of 2 basic views: 1) most expensive cachelines list 2) offsets details for each cacheline

For each cacheline in the 1) list we display following data: (Both stdio and TUI modes follow the same fields output)

    Index
    - zero based index to identify the cacheline

    Cacheline
    - cacheline address (hex number)

    Total records
    - sum of all cachelines accesses

    Rmt/Lcl Hitm
    - cacheline percentage of all Remote/Local HITM accesses

    LLC Load Hitm - Total, Lcl, Rmt
    - count of Total/Local/Remote load HITMs

    Store Reference - Total, L1Hit, L1Miss
      Total - all store accesses
      L1Hit - store accesses that hit L1
      L1Hit - store accesses that missed L1

    Load Dram
    - count of local and remote DRAM accesses

    LLC Ld Miss
    - count of all accesses that missed LLC

    Total Loads
    - sum of all load accesses

    Core Load Hit - FB, L1, L2
    - count of load hits in FB (Fill Buffer), L1 and L2 cache

    LLC Load Hit - Llc, Rmt
    - count of LLC and Remote load hits

For each offset in the 2) list we display following data:

    HITM - Rmt, Lcl
    - % of Remote/Local HITM accesses for given offset within cacheline

    Store Refs - L1 Hit, L1 Miss
    - % of store accesses that hit/missed L1 for given offset within cacheline

    Data address - Offset
    - offset address

    Pid
    - pid of the process responsible for the accesses

    Tid
    - tid of the process responsible for the accesses

    Code address
    - code address responsible for the accesses

    cycles - rmt hitm, lcl hitm, load
      - sum of cycles for given accesses - Remote/Local HITM and generic load

    cpu cnt
      - number of cpus that participated on the access

    Symbol
      - code symbol related to the 'Code address' value

    Shared Object
      - shared object name related to the 'Code address' value

    Source:Line
      - source information related to the 'Code address' value

    Node
      - nodes participating on the access (see NODE INFO section)

NODE INFO

The Node field displays nodes that accesses given cacheline offset. Its output comes in 3 flavors: - node IDs separated by , - node IDs with stats for each ID, in following format: Node{cpus %hitms %stores} - node IDs with list of affected CPUs in following format: Node{cpu list}

User can switch between above flavors with -N option or use n key to interactively switch in TUI mode.

COALESCE

User can specify how to sort offsets for cacheline.

Following fields are available and governs the final output fields set for caheline offsets output:

    tid   - coalesced by process TIDs
    pid   - coalesced by process PIDs
    iaddr - coalesced by code address, following fields are displayed:
               Code address, Code symbol, Shared Object, Source line
    dso   - coalesced by shared object

By default the coalescing is setup with pid,iaddr.

STDIO OUTPUT

The stdio output displays data on standard output.

Following tables are displayed: Trace Event Information - overall statistics of memory accesses

    Global Shared Cache Line Event Information
    - overall statistics on shared cachelines

    Shared Data Cache Line Table
    - list of most expensive cachelines

    Shared Cache Line Distribution Pareto
    - list of all accessed offsets for each cacheline

TUI OUTPUT

The TUI output provides interactive interface to navigate through cachelines list and to display offset details.

For details please refer to the help window by pressing ? key.

CREDITS

Although Don Zickus, Dick Fowles and Joe Mario worked together to get this implemented, we got lots of early help from Arnaldo Carvalho de Melo, Stephane Eranian, Jiri Olsa and Andi Kleen.

C2C BLOG

Check Joe’s blog on c2c tool for detailed use case explanation: https://joemario.github.io/blog/2016/09/01/c2c-blog/

SEE ALSO

perf-record(1), perf-mem(1)